
  _____       _                       _   ____  
  \_   \_ __ | |_ ___  __ _ _ __ __ _| | |___ \ 
   / /\/ '_ \| __/ _ \/ _` | '__/ _` | |   __) |
/\/ /_ | | | | ||  __/ (_| | | | (_| | |  / __/ 
\____/ |_| |_|\__\___|\__, |_|  \__,_|_| |_____|
                      |___/                     
                                             
Have fun. Please share our work around :)
                                                               
**********\ www.HDfury.com /************



*** If Windows GUI does not display nicely:
*** Make sure the GUI isn't already running, then right click the GUI exe file, select "Property"
*** Click the "Compatibility" tab.
*** Look down for "Override high DPI scaling behavior" and check the box.
*** For the drop-down under "Scaling Performed by" choose "System - Enhanced"
*** Start the GUI and revel in how it works normally now.



 _     _  _____   ______  ______ _______ ______  _______
 |     | |_____] |  ____ |_____/ |_____| |     \ |______
 |_____| |       |_____| |    \_ |     | |_____/ |______

### HOW TO UPGRADE ###

If they are not yet installed on your system, please install Silabs driver on your windows computer.

Then simply connect your Vertex unit to your computer via USB, run MCU&FPGA update file and you are done.

After FPGA update, you need to powercycle the Vertex unit and wait about 15s till the update is applied, when OLED turn back ON, the unit is ready to operate.

Updated Version must show: 2.37.2.40 from OSD.

In case of any issue and if the OLED show a lock icon on the top right corner, please HOLD RST and press INP 2 times, unit will prompt for power cycle, after completion and restart, lock isn't present and unit ready to operate without limitations.

User Manual: https://www.hdfury.com/docs/HDfuryIntegral2.pdf




 _______ _     _ _______ __   _  ______ _______              _____   ______
 |       |_____| |_____| | \  | |  ____ |______      |      |     | |  ____
 |_____  |     | |     | |  \_| |_____| |______      |_____ |_____| |_____|


###########> What's new/fixed in 2.37.2.41 / GUI 1.34

1.  When HLG is input but the display does not support HLG then conversion to the current custom HDR string automatically.

2.  GUI selection has two new checkboxes. When HDR10 is input Vertex can automatically replace with the custom metadata. Same thing with HLG input (regardless if display supports it or not)

3.  Fixed issue in autoscaling when sink edid was an old version with HDMI vendor specific string too short, autoscale was decoding value that were not present. 

4.  Fixed Custom Scaling issue that prevented upscaling when sink was max 300MHz and does not contain scramble registers.


###########> What's new/fixed in 2.37.2.37 / GUI 2.33


1. Release version




 ****************************************************
 __  __   ____        ___                             
/\ \/\ \ /\  _`\    /'___\                           
\ \ \_\ \\ \ \/\ \ /\ \__/  __  __   _ __   __  __   
 \ \  _  \\ \ \ \ \\ \ ,__\/\ \/\ \ /\`'__\/\ \/\ \  
  \ \ \ \ \\ \ \_\ \\ \ \_/\ \ \_\ \\ \ \/ \ \ \_\ \ 
   \ \_\ \_\\ \____/ \ \_\  \ \____/ \ \_\  \/`____ \
    \/_/\/_/ \/___/   \/_/   \/___/   \/_/   `/___/> \
                                                /\___/
                                                \/__/
*****************\ www.HDfury.com /*******************


Need a discount code ? Share a link to us, write a review, 
tell people on any forum how cool we are and you will be rewarded with discount code!
the more you do, bigger will be the discount, do something amazing and get a FREE HDFURY!

