 ****************************************************
 __  __   ____        ___                             
/\ \/\ \ /\  _`\    /'___\                           
\ \ \_\ \\ \ \/\ \ /\ \__/  __  __   _ __   __  __   
 \ \  _  \\ \ \ \ \\ \ ,__\/\ \/\ \ /\`'__\/\ \/\ \  
  \ \ \ \ \\ \ \_\ \\ \ \_/\ \ \_\ \\ \ \/ \ \ \_\ \ 
   \ \_\ \_\\ \____/ \ \_\  \ \____/ \ \_\  \/`____ \
    \/_/\/_/ \/___/   \/_/   \/___/   \/_/   `/___/> \
                                                /\___/
                                                \/__/
*****************\ www.HDfury.com /*******************


### HOW TO UPGRADE ###

Simply connect your Android Phone/Tablet to your computer (unlock screen if needed) and make sure you are in storage device mode.
Transfer the APK to your download folder, then access that folder using your mobile/tablet to install the APP.
Use Top Right menu option to clear previous connection if you are having issue to connect to your Vertex device after update.
You can try removing/reinsalling APP in case of issue.

You can also copy Vertex_Commands.xml in your download folder in case you want to use custom menu in your APP (advanced users only)

Updated Version must show: 1.1.0

IMPORTANT: Never pair your phone with Vertex yourself using the Android BT menu. The APP will auto connect and pair on its own. 




### CHANGE LOG ###



//----------------------------------------------------------------------------------------
//	05-Vertex-V1.1.0-2018-06-12 ::UPLOAD
//----------------------------------------------------------------------------------------
	0. Ver name 1.1.0, code = 6
	
	1. For PC GUI v1.31
	
	2. ADD when vertex no connect will show GoBlue version number

//----------------------------------------------------------------------------------------
//	05-Vertex-V1.04-2018-05-09 ::UPLOAD
//----------------------------------------------------------------------------------------
	0. Ver name 1.0.4 , code = 6
	
	1. For PC GUI v1.31
	
	2. CmdID_audioflag add 5=TOP
	
	3. mapping PC Config, App config store at Device Setting 
		audwvol
		audwbass
		audwtreb
		
		Cmd_bvidaud		mapping PC GUI C_VertexCmd_bmtxaudmute / R_Vertex_bmtxaudmute
		Cmd_bvidaud_off
		Cmd_bvidaud_on
		4. modify WriteEditCmd checking "audw!!!" command , for cehck PCB ver if 0 is old pcb,1 is new pcb for allow edit
		
	5. info diplay add PCB_Verion and GoBlue BT MAC address

//----------------------------------------------------------------------------------------
//	05-Vertex-V1.03-2018-02-09 :: UPLOAD
//----------------------------------------------------------------------------------------
	1. Organize unified variables and filenames
	
	2. HDR take off Auto Fill CRC, always Enable, fix before wrhdr make CRC error
	
//----------------------------------------------------------------------------------------
//	05-Vertex-V1.03-2018-02-05
//----------------------------------------------------------------------------------------
	1. support PC GUI v1.13/V1.14
		(a) JVC Macro (GoBlue fix IR receiver)
				CmdID_macroen,
				CmdID_macroen_off,
				CmdID_macroen_on,
				
				CmdID_macrofsh,
				CmdID_macrofsh_off,
				CmdID_macrofsh_on,
				
				CmdID_macromd0,
				CmdID_macromd0_chg,
				CmdID_macromd0_off,
				CmdID_macromd0_on,
				
				CmdID_macromd1,
				CmdID_macromd1_chg,
				CmdID_macromd1_off,
				CmdID_macromd1_on,
				
				CmdID_macromd2,
				CmdID_macromd2_chg,
				CmdID_macromd2_off,
				CmdID_macromd2_on,
				
				CmdID_macromd3,
				CmdID_macromd3_chg,
				CmdID_macromd3_off,
				CmdID_macromd3_on,
				
				CmdID_macromd4,
				CmdID_macromd4_off,
				CmdID_macromd4_on,
				
				CmdID_macromd5,
				CmdID_macromd5_off,
				CmdID_macromd5_on,
				
				CmdID_macromd6,
				CmdID_macromd6_off,
				CmdID_macromd6_on,
				
		(b) Add Auto P0 No Up Scale and MaskGray
				CmdID_p0noup,
				CmdID_p0noup_off,
				CmdID_p0noup_on,
				
				CmdID_osdwmaskgray ~~ 0~15
				

//----------------------------------------------------------------------------------------
//	05-Vertex-V1.02-2018-01-04 :: Upload
//----------------------------------------------------------------------------------------
	1. xml supoort Scale/HDCP checking SWforce
	
	2. Support  Vertex PC GUI v1.08
		(a) DV add 2 setup with 1 Reg, so usage in bit
				Was DV = Bit0
				add CmdID_hdrdvrem ==> DV_Remove = Bit1
				add CmdID_hdrdvlim ==> DV_Limit 300MHz = Bit2
		
		(b) Add 1 Cmd
				ARCHBR	
				add CmdID_cecarc
				
			add 3  Reg
				eArcHbr,
				eScaleSlider ===> replace early eSwState_scale 
				eQuickP,	// not use
				
			add preset mapping table 2 
				Vertex_PRESET_1080P60_444_8,
				Vertex_PRESET_AUTOSENSE,
			
			(1) F_Vx_4k30mode_ItemToID / F_Vx_4k30mode_IDToItem fix was Vertex_PRESET_AUTOSENSE
					Vertex_PRESET_AUTOSENSE default is 0
			(2) F_Vx_4k60mode_ItemToID / F_Vx_4k60mode_IDToItem 
					add Vertex_PRESET_AUTOSENSE / Vertex_PRESET_1080P60_444_8
			(3) F_Vx_4k60hdrmode_ItemToID / F_Vx_4k60hdrmode_IDToItem 
					add Vertex_PRESET_AUTOSENSE / Vertex_PRESET_1080P60_444_8

		(c) Edid and scale change to 2 parameters, not use EdidSw, mapping  eEdidModeSel/eEdidCustom
				eEdidModeSel = NewEdidSw
				eEdidCustom = Custom Mode , its App setup use Reg
				

		(d) Add Never Fade Text, common use R_VxOsdText_en, use Bit mapping
				replace fade on/off
				CmdID_osdfade,
				CmdID_osdfade_off,
				CmdID_osdfade_on,
				mapping Never Fade Text not use  osdfadetime = 0sec/5sec anymore
		
		(e) osd info add video TXRX
				CmdID_osdvidtxrx,
				CmdID_osdvidtxrx_off,
				CmdID_osdvidtxrx_on,
		
		(f) add HTPC Cmd(Avrkey have applied)

//----------------------------------------------------------------------------------------
//	05-Vertex-V1.01-2017-11-21 :: upload
//----------------------------------------------------------------------------------------
	1. ReadAll items number fix, fix auto count, avoid xml items qty (add readAllMaxStep explain xml count)
			for after 2 items
			(a) WrtReadCmd
			(b) ReadCmd
			
	2. add  BaudRate parameter
			CmdID_baud,
			CmdID_baud_0,
			CmdID_baud_1,
			CmdID_baud_2,
			CmdID_baud_3,
	
	3. add RS232 Command input
		
	4. Fix addHexCRC can not use String ,change to use byte [] transmit
			
	5. BLE  change to  1.0.1 version 2
	
//----------------------------------------------------------------------------------------
//	05-Vertex-V1.00-2017-11-13 :: upload
//----------------------------------------------------------------------------------------
	1. external xml change to Vertex_Commands.xml
	
	2. define output formal format  v1.0.0 

/
	
	1. fix edidtab to bm/tp, items 1~100, 0~100
	
	2. fix dtcec
	
	3. fix FW display 
	
	